**Openbmc build commands**

1. if rebuilding the phosphor-dbus-interfaces and don’t see the build, image folder under the *black@bhavin:~/openbmc$ ls build/qemuarm/tmp/work/cortexa15t2hf-neon-openbmc-linux-gnueabi/phosphor-dbus-interfaces/1.0+git/* then execute following commands in build environment
   1. Clean the recipe (remove cached output)

$ bitbake -c cleanall phosphor-dbus-interfaces

* 1. Rebuild it with forced compile

$ bitbake phosphor-dbus-interfaces -f -c compile